Cangzhou Best Machinery Co.,Ltd.&AOFA Machinery Co.,Ltd

ADD: NO.104 Nation Road Songtunzi Village,Botou City,Hebei Province,China

Tel: +86-0317-5205930             Mobile/WhatsApp: +86-18717894416

Email: sales1@chbestmachine.com  website: www.steelrollforming-machine.com
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Main Commercial Terms

	Machine name
	Roof Sheet Roll Forming Machine

	Machine Price
	USD $24,500 FOB Tianjin Port


	Payment term
	30% as down payment by T/T

70% by T/T before loading and after inspection.

	Delivery time
	50 working days since the date of receiving down payment

	Container 
	1x40GP

	Packing
	Main machine naked and fastened with wire rope in the container.All electrics devices be packed with plastic film.

	Warranty
	18 months since the date bill of loading.

	Model
	YX-915-1200

	Machine photo
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	Profile drawing

And product
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Working flow:

Decoiler------feeding------roll forming------cut to length-----output table
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Machine components list:

	Name
	NO.
	Unit

	1.De-coiler
	1
	set

	2.Forming machine
	1
	set

	3.Cutting device
	1
	set

	4.PLC control box
	1
	set

	5.Hydraulic pump station
	1
	set

	6.Production support table
	1
	set
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Main technical parameter:

1.DECOILER 
(1) Max. Width: 1250 mm 
(2) Inner Diameter: Φ450 – Φ550 mm 
(3) Out Diameter: 1500 mm 
(4) Max. Loading Capacity: 5000 kgs

(5)Type: Manual

2. ROLL FORMING MACHINE 
(1) Material Thickness: 0.6-1.5mm PPGI and GI
(2) NO. of roller Stations: 28groups
(3) Material for Rollers: high grade 45# steel polished and coated with chrome HRC55-60°
(4) Material for shaft: high grade 45# steel polished and coated with chrome HRC55-60°
(5) Diameter of shaft: 80mm
(6) Frame panel thickness: 20mm
(7) Bottom frame: 350 H-section steel 
(8) Motor Power: 22kw
(9)Driven type: 2.0＂Chain
(10)Speed:6-8m/min 


3. CUT-OFF DEVICE
(1)Material for Cut-Off Modular:Cr12 steel after treatment
(2)Hardness for Heat Treatment:HRC55 – 60°
(3)Cut-Off Type: Hydraulic, Automatic Cut-Off 
(4) Motor for Hydraulic Stand: 5.5 kW 
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4.PLC CONTROL BOX
(1) Type: PLC Frequency Control System with touch screen 
(2) PLC Brand:Delta
(3) Encoder Brand: Omron
(4)Length Error: ±2mm

(5)Language: English and Chinese
(6)Voltage: 380v/50HZ, 3Phase 

(it depends on customer requirement)

5. HYDRAULIC PUMP STATION

(1) Motor power:5.5 kw
(2)Oil type: 46# hydraulic oil
(3) Pump brand: China brand

6. PRODUCTION SUPPORT TABLE
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(1) No power type
(2)Length: 2m

7.Spare part

Chain x1; Bearing x 1; limit switch x1

	Working conditions

	1.working size
	25m x 2m x 4m

	2.Power supply
	8.5kw

	3.Frequency
	50-60HZ

	4.Wires/cables
	4-6mm²(length according to workshop)

	5. Labor cost
	2 workers

	6. Tools
	Spanners and screwdriver

	7.Lift device
	3-5t forklift or crane


Installation and Training:

① If buyers visit our factory and check the machine, we will teach you how to install and use the machine, and also train your workers/technician face to face.
② Without visiting, we will send you user manual and video to teach you to install and operate.
③If buyer needs our technician to go to your local factory,please arrange round trip tickets, food and hotel and everyday salary USD100, visa cost and necessary things.

